#注释 相关提示，右边为对左边的替换
aatoken=$
apprebsys$Rebuilding app system
burnimage.wr$Buring SD card
comopenfail$Com open failed,retrying...:
comopensuc$Com open success,handshaking...
delpubso$Deleting public SO
dl$Downloading
dlapp.dl$Downloading app
dlapp.wr$Writing app to flash
dlboot$Downloading Boot
dlboot.dl$Downloading Boot
dlboot.er$Erasing Bootflash
dlboot.wr$Writing Bootflash
dlconfig$Downloading system configure file
dlconfig..wr$Writing config to flash
dlconfig.dl$Downloading config
dldriver$Downloading base pos driver
dlfont$Downloading base font
dlfont.dl$Downloading font
dlfont.wr$Writing font to flash
dlhddriv.dl$Downloading head driver
dlhddriv.wr$Writing head driver to flash
dlmddriv.dl$Downloading modual driver
dlmddriv.wr$Writing modual driver to flash
dlmonitor$Downloading monitor
dlmonitor.dl$Downloading monitor
dlmonitor.er$Erasing monitor on flash
dlmonitor.wr$Writing monitor to flash
dlparam.dl$Downloading param
dlparam.wr$Writing param to flash
dlpriso.dl$Downloading private SO file
dlpriso.wr$Writing private SO file
dlpubso.dl$Downloading public SO file
dlpubso.wr$Writing public SO file
dlrambt$Downloading BootRam
dluakey.dl$Downloading uakey
dluakey.wr$Writing uakey to flash
dluskey.dl$Downloading uskey
dluskey.wr$Writing uskey to flash
download$Download
er$Erasing flash
errormsg$Error message
exit_done$Success!
getflash$Get the flash
getflash.check$Handshaking
getflash.image2ftp$Updating image to FTP
getflash.image2mpos$Updating image to remote pos
getflash.openpos$Please connect device and turn on the local pos
putflash.check$handshaking
putflash.crc$crc checking
putflash.done$remote copy completed
putflash.image2flash$Writing flash
putflash.image2pos$Downloading flash
putflash.noimage$the flash mirror of this type not build
putflash.openpos$Please connect device and turn on the remote pos
putflash.waitnext$Task completed,pls change the remote pos for next 
query$Querying the pos infomation
rebsys$Rebuilding the filesystem
removeapp$Removing app
removeapps$Remove all the app
restart$Turn off the device and turn on
setexsn$Setting exsn
setmac$Setting MAC
setprint$Setting the print
setsn$Setting SN
wr$Writing to flash
